|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PRE-QUALIFICATION CRITERIA****Essential and Desirable Facilities required for manufacturing of**

|  |  |  |
| --- | --- | --- |
| **Name of Item & Item Code** | **Essential Facilities** | **Desirable Facilities** |
| "BOLT" (M27 X 1.5-6G) EXCLUDING HARDENING TRACK T-90**Item Code :** 6120100256 | 1. Forging hammer (min. 1 ton) of adequate capacity 2. CNC lathe/ centre lathe 3. Vertical Milling machine/VMC | 1. Heat treatment (austempering) 2. Cadmium plating |

**Other Standard terms and conditions will be as under :*** 1. ‘Firm shall preferably have all the essential facilities in-house’ **or**for any facility which is not with the firm, firm shall produce a MOU with a firm who has the capability and capacity to support the intended tenderer’. In such cases, CV team shall ensure capacity verification of the supporting firm also.
	2. The firm shall have proper quality assurance plan and system to ensure desired level of quality of inputs/ input services.
	3. All the facilities, whether in-house or outsourced should be capable and suitable for producing the items as per specification.

**Note: -** The facilities indicated above are bare essential, better plant and machinery equipment machine is also recommended. |

S