SQUIB EMPTY

PRESS MACHINE,

SURFACE TREATMENT FACILITY (TIN PLATING) OR MOU/TIE-UP WITH SPECIFIED AGENCY FOR SAME, SOLDERING FACILITY,

DRYING FACILITY FOR DRYING AT 90-95 DEG. CENT.