|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PRE-QUALIFICATION CRITERIA**  **Essential and Desirable Facilities required for manufacturing of**   |  |  |  | | --- | --- | --- | | **Name of Item & Item Code** | **Essential Facilities** | **Desirable Facilities** | | NOSE PLUG ARM-1049B(1000 LBS)  **Item Code :** 6220901044 | 1. Forging hammer (min. 1 ton)of adequate capacity 2. Centre Lathe/CNC Lathe 3. Horizontal Milling Machine/Vertical Milling Machine/Vertical Machining Centre | 1.    Chemical testing facility, 2. Mechanical testing facility (UTS, YS, elongation , harness) |   **Other Standard terms and conditions will be as under :**   * 1. ‘Firm shall preferably have all the essential facilities in-house’ **or**for any facility which is not with the firm, firm shall produce a MOU with a firm who has the capability and capacity to support the intended tenderer’. In such cases, CV team shall ensure capacity verification of the supporting firm also.   2. The firm shall have proper quality assurance plan and system to ensure desired level of quality of inputs/ input services.   3. All the facilities, whether in-house or outsourced should be capable and suitable for producing the items as per specification.   **Note: -** The facilities indicated above are bare essential, better plant and machinery equipment machine is also recommended. |